VSP LDF Data file dictionary for IODP Expedition 401 - Hole U1609A

.gmtcommands4 =
.gmtdefaults4 =
401-U1609A_raw_shot_receiver_x.ldf = VSP LDF Data - Raw Shots - X Axis
401-U1609A_raw_shot_receiver_y.ldf = VSP LDF Data - Raw Shots - Y Axis
401-U1609A_raw_shot_receiver_z.ldf = VSP LDF Data - Raw Shots - Z Axis
401-U1609A_raw_shot_source_s1.ldf = VSP LDF Data - Raw Shots - Surface
401-U1609A_raw_stack_receiver_x.ldf = VSP LDF Data - Raw Stacks - X Axis
401-U1609A_raw_stack_receiver_y.ldf = VSP LDF Data - Raw Stacks - Y Axis
401-U1609A_raw_stack_receiver_z.ldf = VSP LDF Data - Raw Stacks - Z Axis
401-U1609A_wavefield_receiver_x.ldf = VSP LDF Data - Wavefield - X Axis
401-U1609A_wavefield_receiver_y.ldf = VSP LDF Data - Wavefield - Y Axis
401-U1609A_wavefield_receiver_z.ldf = VSP LDF Data - Wavefield - Z Axis